1. Materials for thermal socks:

1) covering thread (cotton yarn 30 tex) - 0,062kg (100% combed cotton Ne20\1 або Nm34\1 ) - 630 kg.

2) basic thread ( textured PA thread with eleastanovy rod thread (type Е22+ПА78dtex) to 8,8 tex) - 0,012 kg (PA78SP22 ACY (air covered yarn) - 125 kg.

3) Thread on board and bandage (elastane thread with double braiding PA thread (type Е130+PA78dtex) to 150 tex) - 0,006 kg (rubber El130 spun covered with PA78) 90 kg.

2. Materials for demi-season underwear (briefs + t-shirt + blouse + pants).

Width of running meter in all cloths 1,5 m

1) knitted cloth, composition - 95% cotton 5% elastane, density - 160g/m2 (elastic knitted fabric, composition - 95% cotton 5% elastane, thiсkness - 160 g/m2) 28000 r.m.

2) knitted cloth, composition - 95% cotton 5% elastane, density - 170г/м2 (elastic knitted fabric, composition - 95% cotton 5% elastane, thiсkness - 170 g/m2) 2500 r.m.

3) knitted cloth, composition - 95% cotton 5% elastane, density - 170г/м2 (elastic knitted fabric, composition - 95% cotton 5% elastane, thiсkness - 170 g/m2) 8000 r. m.

4) elastic rubber underwear, Width 30 mm (elastic band for underwear, width - 30 mm) - 18000 m.

5) Thread Epic tkt 120 (5000m) the same as a cloth color - 330 bobbins

6) Thread Gramax tkt 160(10000m) the same as a cloth color - 370 bobbins